2022-11-13
Hall: GA Booth: 73

ESSEN MOTOR SHOW

Powerdrop adhesives

PowerDrop adhesives are modified reactive adhesives (cyanoacrylates). They are applied in liquid form and, under suitable conditions, react to form solids (curing). The cured adhesive is a plastic. Depending on the material, the adhesive surfaces harden quickly. Smooth within a short time (glass, metal, plastic, rubber) - porous after just a few minutes (wood, leather, porcelain, ceramics, clay). Different materials can also be bonded without any problems. The gap filling capacity is maximum 0.25 millimetre For larger gap widths, PowerDrop fillers are recommended.

Application areas:
Its adhesion to most materials is excellent and its adhesive strength under shear and tensile stress is very good. PowerDrop adhesives are largely water, lye, oil, grease, UV, light, heat and cold resistant.

Processing:
As a minimum requirement for surface treatment, is recommended: Oil, grease or other layers (old glue, rust) must be removed (with PowerDrop Remover). Apply a thin layer of PowerDrop to one side, press together, leave for a few seconds and then allow to harden for some time, depending on whether the surface is porous or smooth. This item may only be used in accordance with the manufacturer's instructions/operating instructions. Read the manufacturer's instructions and observe the product or safety data sheet.

Contact:
Powerdrop Industrieklebstoffe
Herr Johann Hödl
Philipsstraße 26
8403 Lebring
Austria
Fon: +4369981290969
E-Mail: powerdrop1@gmail.com
----------------------------------------