2022-06-01
Hall: 7 Booth: 7A43

IPM Summer Edition

Power drive EWA 50

· Extremely quiet, self-locking double worm gear with integrated end position shutdown and with long service life, maintenance-free

· Universal mounting due to standard mounting at the rear or side left (symmetrical)

· Standard foot mount with 70mm center distance or optional 60 milimetre

· End position limit control unit LSC 40AC/DC incl. additional limit switch; optional precision gear limit switch END 20

· Single-phase motors pre-wired with connection cable and integrated winding protection contact

· Replacement compatible with EWA10/12

Contact:
Lock Antriebstechnik GmbH
Frau Corina Wetzel
Freimut-Lock-Str. 2
88521 Ertingen
Germany
Fon: +49737195080
Fax: +497371950880
E-Mail: cwe@lcokdrives.com
----------------------------------------