2018-11-19
Hall: 8 Booth: 8C22

ESSEN MOTOR SHOW

Comp. Intercooler Kit Honda Civic Type R FK8

The Wagner Tuning high-performance intercooler has got a new competition core (Tube Fin) with the dimensions 670 x 183,4 x 125 millimetre (15.4 liters)/ 26,38 x 7,22I x 4,92 Inch (939,76 Inch³), which was developed especially for the requirements of the Honda Civic Type R FK8. This high-performance core offers an 23 percent larger frontal surface and 140 percent more core volume compared to the stock intercooler.

The aluminum cast endtanks were designed in CAD and optimized in CFD simulations (for an ideal internal airflow). An incorporated air baffle inside the intercooler inlet ensures a uniform filling of the intercooler. The result is an excellent cooling property with a minimal back pressure. The newly developed competition high-performance core is very light and provides the adjoining components (for example the watercooler) enough air flow by using a specially prepared air baffle. That is why this kit is perfect for racing use. An optimal cooling effect of the charged air with a significant increase in performance.

An anti-corrosion powder coating with perfect heat-conducting properties protects the Wagner Tuning intercooler from all environmental influences, so a lasting and optimal cooling effect can be guaranteed. The installation is done by replacing the original intercooler and is easy to perform (plug and play). 

Inlet diameter: 65 millimetre / 2,56 Inch; outlet diameter 70 millimetre / 2,75 Inch

Dimensions stock intercooler:
V = 6,4 L / 239,55Inch³
A = 6403200 mm²/ 9 925 Inch²

Dimensions WAGNERTUNING intercooler:
V = 15,4 L / 939,76Inch³
A = 15359750 mm²/ 23 808 Inch²

kit comes with:
1 intercooler
1 air baffle
2 silicone hoses (black)
1 mounting material
1 installation instruction

Contact:
Wagner Tuning
Herr Ben Naumann
Mittelbreite 11-13
06861 Dessau-Roßlau
Germany
Fon: +493490159700
E-Mail: info@wagner-tuning.de
----------------------------------------